**ALL ITEMS NEEDING ATTENTION MUST BE ACTIONED AND RESOLVED**

| **Hazards** | **OK** | **Needs Attention** | **Action/ Notes** |
| --- | --- | --- | --- |
| **Cotton Pickers** | | | |
| All pickers are turned off and keys removed before servicing or maintenance |  |  |  |
| All moving parts are guarded and guards kept in place |  |  |  |
| Hydraulic cylinder locks and/or other blocks and chocks used to support raised picker heads, baskets or other equipment when it is required to work underneath them |  |  |  |
| Are picker baskets raised ‘over centre’ to prevent baskets falling when servicing pickers |  |  |  |
| Picker baskets lowered and locked so they cannot be raised during picker transport |  |  |  |
| Steps and handrails are undamaged and prevent operators falling |  |  |  |
| Fall arrest systems are used when working on or cleaning picker baskets |  |  |  |
| Lights, reflectors, wind screens and mirrors are undamaged and kept clean |  |  |  |
| Operators seats on cotton pickers are undamaged and in good condition |  |  |  |
| A First Aid kit is carried on all cotton pickers |  |  |  |
| A fire extinguisher mounted on each cotton picker |  |  |  |
| **Module Builders** |  |  |  |
| Hydraulic motors or tractor PTO is disengaged, motors stopped and keys removed before any worker gets inside or services module builders |  |  |  |
| Trampers and rams are lowered before transport to avoid electrocution |  |  |  |
| All module builders have a shade canopy or cabin over the operator’s seat and controls |  |  |  |
| Safe transport routes have been established for the movement of module builders |  |  |  |
| High visibility clothing or reflective vests and torches are available for module builder operators and ground crew when picking at night |  |  |  |
| Ear muffs or plugs are worn by module builder operators |  |  |  |
| Dust masks available for module builder operators and ground crew |  |  |  |
| A First Aid kit Is available near the operating environment of the module builder and ground crew |  |  |  |
| There is a fire extinguisher mounted on all module builders |  |  |  |
| There is good lighting for night operations |  |  |  |
| **Boll Buggies** | | | |
| Hydraulic motors or tractor PTO is disengaged, motors stopped and keys are removed before any worker gets inside or services boll buggies |  |  |  |
| Hydraulic cylinder locks and/or other blocks and chocks used to support raised boll buggy baskets or when it is required to work underneath them |  |  |  |
| A First Aid kit Is available on tractors towing boll buggies |  |  |  |
| There is a fire extinguisher mounted on all tractors |  |  |  |
| There is good lighting for night operations |  |  |  |
| High visibility clothing is worn when picking at night |  |  |  |
| **Telehandlers** | | | |
| All operators are properly trained to use telehandlers and transport modules. |  |  |  |
| Telehandlers are regularly checked that all pins and locking pins are in place. |  |  |  |
|  |  |  |  |
|  |  |  |  |