**ALL ITEMS NEEDING ATTENTION MUST BE ACTIONED AND RESOLVED**

| **Hazards** | **OK** | **Needs****Attention** | **Notes** |
| --- | --- | --- | --- |
| **Cherry Pickers** |  |
| All operators are properly trained to use cherry pickers |  |  |  |
| All cherry pickers are serviced and maintained according to manufacturer’s safety directions |  |  |  |
| A preoperational check of controls and safety systems (brakes, hydraulics and pins) is conducted before each days use |  |  |  |
| All cherry pickers are inspected and maintained as described in Annex 1 of the Australian/NZ Standard 2550.10 *Cranes, hoists and winches Part 10: Mobile elevating work platforms* |  |  |  |
| All picking bags are in good repair |  |  |  |
| The size of picking bags is appropriate for the Safe Weight Limit (SWL) and do not overload the cherry picker |  |  |  |
| Safety harness and harness attachments (where an assessment has been made for their use) are used and in good condition  |  |  |  |
| Hand controls are guarded to prevent tree branches and limbs activating controls |  |  |  |
| Foot controls are covered to prevent fruit jamming under the controls |  |  |  |
| Cherry picker baskets are kept clean to prevent fruit and debris jamming foot controls |  |  |  |
| **Additional Hazards** |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |